NVM Express Controller
======================

The nvme device (-device nvme) emulates an NVM Express Controller.


Reference Specifications
------------------------

The device currently implements most mandatory features of NVMe v1.3d, see

  https://nvmexpress.org/resources/specifications/

for the specification.


Known issues
------------

* The accounting numbers in the SMART/Health are reset across power cycles

* Interrupt Coalescing is not supported and is disabled by default in volation
  of the specification.
